PLEASE NOTE: The following specification contains areas, highlighted with the [ ] symbol. In these areas, the engineer has to make a selection, add specific, project related information and has to delete what is not applicable for the specific project.
ORP Sensor
Online process ORP sensor with built in temperature probe for measuring oxidation/reduction potential of water at high temperature. The sensor connects to a digital controller for operation.
Technical Data
Application
ORP at high temperature
Junction type
Flat, PTFE
Material
Reference Electrode: Ag/AgCl
Measuring range
-1500 mV - 1500 mV
Operating temperature range

0 - 110 °C
Pressure range
Max. 10 bar at 80 °C
Drift
<3 mV/week
Offset @ pH 7
N/A
Slope Range
N/A
Impedance
Reference impedance @ 25 °C: <50 kΩ
Glass impedance @ 25 °C: Platinum
Weight
0.62 kg
Scope of delivery
[ ] (delete what is not needed)
Sensor comes with a 10 m cable and manual
Accessories
[ ] PVC DN 40 flow chamber, flange fitting
[ ] PP immersion shaft, clip fitting (0.5, 1, 1.5 meter)
[ ] PP immersion shaft, adjustable flange (0.5, 1, 1.5 meter) [ ] PP immersion shaft, fixed flange (0.5, 1, 1.5 meter)
[ ] PP chemical cleaning kit (nozzle and feed pipes) [ ] Liquid reservoir unit
[ ] Junction box
[ ] Low-impedance cable, type 2666
[ ] High-impedance co-axial cable, type 2654
Services
[ ] Manufacturer’s services to perform start-up on instrument to include basic operational training and certification of
performance of the instrument.
[ ] Manufacturer’s Service Agreement that covers all the manufacturer’s recommended preventative maintenance, regularly scheduled calibration and any necessary repairs beginning from the time of equipment start-up through to end user acceptance / plant turnover and the first 12 months of end-user operation post turnover.
Brand:
Polymetron
Product:
8351 ORP Sensor
