# NGMP Cond Default method Configurable parameters
# Name			|Value|Default		|lType		|Name2				|Limits
#==========================================================================================
#
version			|	|3				|ecRange	|					|1:99
parameter		|	|_440			|ecStrings	|_401			|_440		:_441		:_442		:_443		
# Measurement Options:  
# Conductivity MxOption
cdtvtyUnitTyp	|	|_411			|ecStrings	|_439				|_411		:µS/cm:mS/cm
cdtvtyLowAutoLP	|	|0.01 µS/cm		|ecFloat	|_272				|0.01 µS/cm:199999.00 µS/cm
cdtvtyHighAutoLP|	|200000.00 µS/cm|ecFloat	|_273				|0.02 µS/cm:200000.00 µS/cm
cdtvtyLowAutoMP	|	|0.01 µS/cm		|ecFloat	|_272				|0.01 µS/cm:399999.00 µS/cm
cdtvtyHighAutoMP|	|400000.00 µS/cm|ecFloat	|_273				|0.02 µS/cm:400000.00 µS/cm
cdtvtyLowuSLP	|	|0.01 µS/cm		|ecFloat	|_272				|0.01 µS/cm:9998.00 µS/cm
cdtvtyHighuSLP	|	|9999.00 µS/cm	|ecFloat	|_273				|0.02 µS/cm:9999.00 µS/cm
cdtvtyLowuSMP	|	|0.01 µS/cm		|ecFloat	|_272				|0.01 µS/cm:9998.00 µS/cm
cdtvtyHighuSMP	|	|9999.00 µS/cm	|ecFloat	|_273				|0.02 µS/cm:9999.00 µS/cm
cdtvtyLowmSLP	|	|0.200 mS/cm	|ecFloat	|_272				|0.200 mS/cm:199.999 mS/cm
cdtvtyHighmSLP	|	|200.000 mS/cm	|ecFloat	|_273				|0.201 mS/cm:200.000 mS/cm
cdtvtyLowmSMP	|	|0.200 mS/cm	|ecFloat	|_272				|0.200 mS/cm:399.999 mS/cm
cdtvtyHighmSMP	|	|400.000 mS/cm	|ecFloat	|_273				|0.201 mS/cm:400.000 mS/cm
temperCompensTyp|	|_419			|ecStrings	|_412				|_417		:_418			:_419		:_420			
temperCorrFactor|	|1.90 %/°C		|ecFloat	|_414				|0.00 %/°C:9.99 %/°C
temperReference	|	|25 °C			|ecStrings	|_428				|20 °C:25 °C
# Salinity MxOption hierarchy
salinityUnit	|	|_465			|ecStrings	|_406				|_465	:_484	:g/kg:_408						# per 1000, g/kg, <unitless> 
slnityLowNoUnit	|	|0.0			|ecFloat	|_272				|0.0:41.9  # (no unit)
slnityHighNoUnit|	|42.0			|ecFloat	|_273				|0.1:42.0  # (no unit)
slnityLowPerMil	|	|0.0 _465		|ecFloat	|_272					|0.0 _465	:41.9 _465	
slnityHighPerMil|	|42.0 _465	|ecFloat	|_273					|0.1 _465	:42.0 _465	
slnityLowppt	|	|0.0 ppt	|ecFloat	|_272					|0.0 ppt:41.9 ppt
slnityHighppt	|	|42.0 ppt	|ecFloat	|_273					|0.1 ppt:42.0 ppt
slnityLowGperkg	|	|0.0 g/kg		|ecFloat	|_272				|0.0 g/kg:41.9 g/kg
slnityHighGperkg|	|42.0 g/kg		|ecFloat	|_273				|0.1 g/kg:42.0 g/kg
# Total Dissolved Solids MxOption
tdsLowLimit		|	|0 mg/L			|ecRange	|_272				|0 mg/L:49999 mg/L
tdsHighLimit	|	|50000 mg/L		|ecRange	|_273				|1 mg/L:50000 mg/L
# Resistivity MxOption
rstvityLowLimLP|	|5.0_473		|ecFloat	|_272				|5.0_473		:49999900.0_473		
rstvityHighLimLP|	|50000000_473		|ecFloat|_273			|5.1_473		:50000000.0_473		
rstvityLowLimMP|	|2.5_473		|ecFloat|_272				|2.5_473		:49999900.0_473		
rstvityHighLimMP|	|50000000_473		|ecFloat|_273			|2.6_473		:50000000.0_473		
# Menu Cal Options
calStds			|	|NaCl, 1000µS/cm - 25°C|ecStrings|_421			|1D KCl, 111.3mS/cm - 25°C:0.1D KCl, 12.85mS/cm - 25°C:0.01D KCl, 1408µS/cm - 25°C:0.1M KCl, 12.88mS/cm - 25°C:0.01M KCl, 1413µS/cm - 25°C:0.001M KCl, 146.93µS/cm - 25°C:NaCl, 18mS/cm - 25°C:NaCl, 1000µS/cm - 25°C:NaCl, 180µS/cm - 25°C:NaCl, 25µS/cm - 25°C:NaCl .05%, 1015µS/cm - 25°C:_460			:_461		
calRemindRepeat	|	|_30			|ecStrings	|_304				|_30:2 h:4 h:8 h:2 d:5 d:7 d
calExpires		|	|_261		|ecStrings	|_277				|_260		:_261		:_262		:_263			:_264			
#calMin			|	|1				|ecStrings	|_278				|1:2:3
#tempCompensCoef|	|1.10 %/°C		|ecFloat	|_430				|0.00 %/°C:9.99 %/°C
stdCustomValue	|	|1000 µS/cm		|ecRange	|_466				|1 µS/cm:199999 µS/cm
stdCustomRefTemp|	|25 °C			|ecSigned	|_428				|-10 °C:+110 °C
stdCustomCoef	|	|1.90 %/°C		|ecFloat	|_430				|0.00 %/°C:9.99 %/°C
checkStandard	|	|NaCl, 1000µS/cm - 25°C|ecStrings|_421			|1D KCl, 111.3mS/cm - 25°C:0.1D KCl, 12.85mS/cm - 25°C:0.01D KCl, 1408µS/cm - 25°C:0.1M KCl, 12.88mS/cm - 25°C:0.01M KCl, 1413µS/cm - 25°C:0.001M KCl, 146.93µS/cm - 25°C:NaCl, 18mS/cm - 25°C:NaCl, 1000µS/cm - 25°C:NaCl, 180µS/cm - 25°C:NaCl, 25µS/cm - 25°C:NaCl .05%, 1015µS/cm - 25°C:_460			:_461		
chkstdCustomValue|	|1413 µS/cm		|ecRange	|_466				|1 µS/cm:199999 µS/cm
chkstdCustomRefTemp||25 °C			|ecSigned	|_428				|-10 °C:+110 °C
chkstdCustomCoef|	|1.90 %/°C		|ecFloat	|_430				|0.00 %/°C:9.99 %/°C
stdRemindRepeat	|	|_30			|ecStrings	|_304				|_30:30 min:2 h:4 h:8 h:12 h:24 h
stdDefer		|	|_22			|ecStrings	|_283				|_22:_21
stdLimits		|	|8 %			|ecRange	|_284				|1 %:9 %
stdFailExpiresCal|	|_21			|ecStrings	|_285				|_22:_21
#
# JYC: for Lab and/orHP
stabilityCritHP	|	|1.0 %/min		|ecFloat	|_462			|0.1 %/min:99.9 %/min
pureWaterOffset	|	|_30			|ecOption	|_0					|_29:_30
#Added by BHa in version 2
tdsFactor		|	|0.500			|ecFloat	|_474			|0.050:5.000
tdsFactorType	|	|NaCl			|ecStrings	|_475			|NaCl:_461		
#Added by JYC in version 3 (Sparky REQCDC1.2.1 & REQCDC1.2.2)
stdCustomUnits	|	|µS/cm			|ecStrings	|_479				|µS/cm:mS/cm
stdCustomValmS	|	|1.000 mS/cm	|ecFloat	|_466				|0.001 mS/cm:199.999 mS/cm
chkstdCustomUnits|	|µS/cm			|ecStrings	|_479				|µS/cm:mS/cm
chkstdCustomValmS|	|1.413 mS/cm	|ecFloat	|_466				|0.001 mS/cm:199.999 mS/cm
#ck 
